BasinInfo               Data sample: characteristics of a different
                        catchments
BasinObs                Data sample: time series of observations of
                        different catchments
Calibration             Calibration algorithm that optimises the error
                        criterion selected as objective function using
                        the provided functions
Calibration_Michel      Calibration algorithm that optimises the error
                        criterion selected as objective function using
                        the Irstea procedure described by C. Michel
CreateCalibOptions      Creation of the CalibOptions object required
                        but the Calibration* functions
CreateErrorCrit_GAPX    Creation of the ErrorCrit_GAPX function
CreateIniStates         Creation of the IniStates object possibly
                        required by the CreateRunOptions functions
CreateInputsCrit        Creation of the InputsCrit object required to
                        the ErrorCrit functions
CreateInputsCrit_Lavenne
                        Creation of the InputsCrit object for Lavenne
                        Criterion
CreateInputsModel       Creation of the InputsModel object required to
                        the RunModel functions
CreateRunOptions        Creation of the RunOptions object required to
                        the RunModel functions
DataAltiExtrapolation_Valery
                        Altitudinal extrapolation of precipitation and
                        temperature series described by A. Valery
ErrorCrit               Error criterion using the provided function
ErrorCrit_KGE           Error criterion based on the KGE formula
ErrorCrit_KGE2          Error criterion based on the KGE' formula
ErrorCrit_NSE           Error criterion based on the NSE formula
ErrorCrit_RMSE          Error criterion based on the RMSE
Imax                    Computation of the maximum capacity of the GR5H
                        interception store
PE_Oudin                Computation of series of potential
                        evapotranspiration at the daily or hourly time
                        steps with Oudin's formula
Param_Sets_GR4J         Generalist parameter sets for the GR4J model
RunModel                Run with the provided hydrological model
                        function
RunModel_CemaNeige      Run with the CemaNeige snow module
RunModel_CemaNeigeGR4H
                        Run with the CemaNeigeGR4H hydrological model
RunModel_CemaNeigeGR4J
                        Run with the CemaNeigeGR4J hydrological model
RunModel_CemaNeigeGR5H
                        Run with the CemaNeigeGR5H hydrological model
RunModel_CemaNeigeGR5J
                        Run with the CemaNeigeGR5J hydrological model
RunModel_CemaNeigeGR6J
                        Run with the CemaNeigeGR6J hydrological model
RunModel_GR1A           Run with the GR1A hydrological model
RunModel_GR2M           Run with the GR2M hydrological model
RunModel_GR4H           Run with the GR4H hydrological model
RunModel_GR4J           Run with the GR4J hydrological model
RunModel_GR5H           Run with the GR5H hydrological model
RunModel_GR5J           Run with the GR5J hydrological model
RunModel_GR6J           Run with the GR6J hydrological model
RunModel_Lag            Run with the Lag model
SeriesAggreg            Conversion of time series to another time step
                        (aggregation only) and regime computation
TransfoParam            Transformation of the parameters using the
                        provided function
airGR-package           Suite of GR Hydrological Models for
                        Precipitation-Runoff Modelling
plot                    Default preview of model outputs
